[15:24:15] 

[15:24:16] eGalaxUpdate2 v3.0.8.7 (221117.154.154) -Demo
[15:24:16] eGalaxUpdate2 Initialized.
[15:24:16] Find touch controller: P80H83
[15:24:16] - Type: PCAP80H83 Series
[15:24:16] - Model: Orion_0592_0185
[15:24:16] - Version: F1_D00_M01
[15:24:16] - ModelInfo: DefFlash
[15:24:16] Controller get EHQA level : 0x00
[15:24:16] Touch controller connected.
[15:24:23] Image Type: P80H83
[15:24:23] FW image get EHQA level : 0x00
[15:24:23] Load Image OK
[15:24:25] Reset controller Pass.
[15:24:25] Wait controller disconnect.
[15:24:25] Device disconnected for PnP process.
[15:24:25] Wait controller disconnect success.
[15:24:26] Wait controller PnP process.
[15:24:27] Find touch controller: P80H83 Loader
[15:24:27] - Status Code: 0x4000
[15:24:27] - Type: P80H83 Series
[15:24:27] - Model: P80H83 BFW
[15:24:27] - Version: 1.14
[15:24:27] - ModelInfo: N/A
[15:24:27] Touch controller PnP Success.
[15:24:27] Check loader state Pass.
[15:24:31] Erase firmware Pass.
[15:24:31] Download firmware.
[15:24:31] Downloading... 08%
[15:24:32] Downloading... 17%
[15:24:32] Downloading... 27%
[15:24:33] Downloading... 36%
[15:24:33] Downloading... 46%
[15:24:34] Downloading... 55%
[15:24:34] Downloading... 65%
[15:24:35] Downloading... 74%
[15:24:35] Downloading... 83%
[15:24:36] Downloading... 92%
[15:24:36] Download firmware Pass.
[15:24:36] Verify download result Pass.
[15:24:36] Reset controller Pass.
[15:24:36] Wait controller disconnect.
[15:24:37] Device disconnected for PnP process.
[15:24:37] Wait controller disconnect success.
[15:24:37] Wait controller PnP process.
[15:24:38] Find touch controller: P80H83
[15:24:38] - Type: PCAP80H83 Series
[15:24:38] - Model: Orion_0592_0185
[15:24:38] - Version: F1_D00_M01
[15:24:38] - ModelInfo: DefFlash
[15:24:38] Controller get EHQA level : 0x00
[15:24:38] Touch controller PnP Success.
[15:24:39] Check firmware state Pass.
[15:24:39] Verfication Pass.
[15:24:43] 
**** eGalaxSensorTester.csv Start ****

[15:24:44] [   0.047] DiagFreq=176.470KHz
[   0.062] Check DC Calib Success
[   0.078] IC0 Calibrating Value =100
[   0.109] Calibration Pass
[15:24:44] 
**** eGalaxSensorTester.csv End ****

[15:24:44] Check calibration setting file: Pass!
[15:24:48] Hardware calibration Pass.
[15:24:48] Reset firmware Pass.
[15:24:48] Firmware update Success.
[15:24:51] Application Exit
[15:24:51] Firmware update resource release.
